|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| WhatsApp Image 2024-09-19 at 11 | **DCS ENGINEERS & CONSULTANT Pvt. Ltd.**  **(Formerly known as DC Consultant)**  Mobile : +91-7018819894, +91-9816755805, e-mail : [officialdcspvtltd@gmail.com](mailto:officialdcspvtltd@gmail.com)  **Regd. Office : VPO Taragarh (Rani Di K) Near Taragarh Palace Tehsil Baijnath District Kangra Himachal Pradesh (176081)** | | | | | |
| **Sieve Analysis** | **ANALYSIS DATA SHEET QSF-1001** | | | | | |
| Job Card No: | | | | Test: | | |
| Sample Description: | | | | Method: | | |
| DOR: | | DOS: | | DOC: | | Page No: |
| Sample Qty: | | | Residual Sample: | | Sample Retention: | |

|  |
| --- |
|  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **GRAIN SIZE ANALYSIS OF SOIL**  **(As Per IS : 2720, Part- 4)** | | | | |
| IS SIEVE (mm). | Weight Retained (gms) | Cumulative Wt. Retained (gms) | Cumulative % Retained | % of Passing |
|  |
| 100 mm |  |  |  |  |  |
| 75 mm |  |  |  |  |  |
| 20 mm |  |  |  |  |  |
| 10 MM |  |  |  |  |  |
| 4.75 mm |  |  |  |  |  |
| 2.0 mm |  |  |  |  |  |
| 425 µ |  |  |  |  |  |
| 75 µ |  |  |  |  |  |
|  |  |  |  |  |  |
| Gravel Content =\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ % | | | |  |  |
|  | |  |  |  |  |
| Sand Contant =\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% | | | |  |  |
|  |  |  |  |  |  |
| Silt & Clay Contant =\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_% | | | |  |
|  |  |  |  |  |  | |

**Checked by Analyst**