|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| WhatsApp Image 2024-09-19 at 11 | **DCS ENGINEERS & CONSULTANT Pvt. Ltd.**  **(Formerly known as DC Consultant)**  Mobile : +91-7018819894, +91-9816755805, e-mail : [officialdcspvtltd@gmail.com](mailto:officialdcspvtltd@gmail.com)  **Regd. Office : VPO Taragarh (Rani Di K) Near Taragarh Palace Tehsil Baijnath District Kangra Himachal Pradesh (176081)** | | | | | |
| **A.C.V.** | **ANALYSIS DATA SHEET QSF-1001** | | | | | |
| Job Card No: | | | | Test: | | |
| Sample Description: | | | | Method: | | |
| DOR: | | DOS: | | DOC: | | Page No: |
| Sample Qty: | | | Residual Sample: | | Sample Retention: | |

|  |
| --- |
|  |

|  |
| --- |
| **(AGGREGATE CRUSHING VALUE)** |

**Aggregate Crushing Value [IS 2386 (Part-4)-1963 RA 2016]**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Aggregate  Size (mm) | Wt. of Container (gm) | Wt. Of  Container + Aggregate (gm) | Wt. Of Aggregate  before Crushing (gm) | Wt. of Aggregate retained on 2.36 mm Sieve (gm) | Wt. of Aggregate Passing from 2.36 mm Sieve (gm) | Aggregate Crushing Value % |
|
|  | **1** | **2** | **3=2-1** | **4** | **5** | **6=(5/3)x100** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |
| **AVERAGE** | | | | | |  |

**Checked by Analyst**