|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| WhatsApp Image 2024-09-19 at 11 | **DCS ENGINEERS & CONSULTANT Pvt. Ltd.**  **(Formerly known as DC Consultant)**  Mobile : +91-7018819894, +91-9816755805, e-mail : [officialdcspvtltd@gmail.com](mailto:officialdcspvtltd@gmail.com)  **Regd. Office : VPO Taragarh (Rani Di K) Near Taragarh Palace Tehsil Baijnath District Kangra Himachal Pradesh (176081)** | | | | | |
| **Paver Block** | **ANALYSIS DATA SHEET QSF-1001** | | | | | |
| Job Card No: | | | | Test: | | |
| Sample Description: | | | | Method: | | |
| DOR: | | DOS: | | DOC: | | Page No: |
| Sample Qty: | | | Residual Sample: | | Sample Retention: | |

|  |
| --- |
|  |

**Age of Specimen:**

**Area Calculation: Asw= 20000 MSP MM2**

**MSTD**

|  |  |  |  |
| --- | --- | --- | --- |
| **S.NO** | **AREA (MM2)** | **LOAD (KN)** | **COMPRESSIVE STRENGTH (N/MM2)** |
|  | A | L | CS = L/A X 1000 |
| 1 |  |  |  |
| 2 |  |  |  |
| 3 |  |  |  |
| 4 |  |  |  |
| 5 |  |  |  |
| 6 |  |  |  |
| 7 |  |  |  |
| 8 |  |  |  |
| **AVERAGE VALUE** | | |  |
| **As Per IS 15658 : 2006 from Table No. 5 Correction factor for............................mm thick**  **................................... Block is........................** | | | |
| **CORRECTED VALUE(Average Value × C.F) =** | | |  |

**Checked by Analyst**